=============== Read This First===============

VersaPro 2.04 configures and programs the following GE Fanuc PLCs : VersaMax, VersaMax
Nano and Micro, Series 90 Micro, the entire family of Series 90-30 PLCs, and the Series
90-70 PLCs.

VersaPro runs under Windows 95/98, Windows NT, Windows 2000, Windows Millennium Edition(Me),
and Windows XP Professional.

VersaPro 2.04 also includes release 2.04 of the Remote I/O Manager software
used to configure VersaMax Network Interface Units (NIUs) and their associated I/O.

VersaPro provides Instruction List (IL) and Relay Ladder Diagram (RLD) programming 
editors for creation of logic, an easy-to-use graphical hardware configuration package, 
and a powerful set of diagnostic and troubleshooting tools. VersaPro also allows users 
of Logicmaster 90-30, Logicmaster 90-70 and Control to import their existing programs.

VersaPro software is designed to be easy to use - that means that you can 
configure a PLC, write logic, connect and store to a PLC within 5 minutes - without 
ever using a manual!

The information that follows provides important useful information regarding the use 
of VersaPro.  Please read this information before using the product.  There is also
a file on the CD titled, "tutorial.pdf", which is useful for first time users.

=============== Important Product Information ===============

For the most up to date information about VersaPro please read the Important Product 
Information document (GFK-1671) included with this product.  This document exists 
in electronic form as a Microsoft Word document on the VersaPro CD, and a paper copy 
is included in the original packaging for the VersaPro product.

=============== Installing VersaPro Release 2.04 ===============

1. System Requirements:

	Windows 95B/98
		486/66Mhz Minimum;  Pentium 133Mhz Recommended
		16MB Minimum; 32MB Recommended
	Windows NT
		486/66Mhz Minimum;  Pentium 133Mhz Recommended
		24MB Minimum; 64MB Recommended
	Windows 2000
		Pentium 2 Minimum;  Pentium 3 Recommended
		64MB Minimum; 128MB Recommended
	Windows Millennium Edition(Me)
		Pentium 150 Mhz Minimum; Pentium 3 Recommended
		64MB Minimum; 128MB Recommended
	Windows XP Professional
		Pentium 233 Mhz Minimum; Pentium 300 Mhz Recommended
		64MB Minimum; 128MB Recommended

	Operating systems supported:  
		Windows 95B
		Windows 98 (First Edition Service Pack 1, Second Edition)
		Windows NT 4.0 (Service Pack 5, Service Pack 5 international version, 
			Service Pack 6)
		Windows 2000
		Windows Millennium Edition(ME)
		Windows XP Professional
	36 MB Hard Disk Space
	50 MB Free Hard Disk Space when running the VersaPro application
	VGA Monitor
	CD ROM Drive
2. Put the VersaPro CD in CD-ROM Drive.
3. Select the CD drive from Windows Explorer.
4. Double click Setup.exe 
5. Follow the user prompts to install your software.

Note:  In some instances, users with CIMPLICITY HMI, Control or GE Fanuc's Host 
Communication Toolkit installed on their computer will be prompted to replace 
"shared files" during the installation. To ensure necessary system files are 
not removed from the system, always select the "No to All" button.  

=============== Starting the VersaPro application ===============

The VersaPro application is installed in the GE Fanuc Software Program group.  The 
application can be started by selecting Start|GE Fanuc Software|VersaPro|VersaPro.  
Users can create a shortcut to the VersaPro application and place the shortcut on 
the desktop, or click on a file created by VersaPro (the file in the VersaPro 
folder with a .fld extension), and start the application in the context of the 
selected folder.
VersaPro can also be started by pressing Ctrl-Alt-V.

=============== VersaPro Manual On-Line ===============

The VersaPro Users Guide (GFK-1670) is included on the CD in a Adobe Acrobat (.PDF) 
format.  If you already have the Adobe Acrobat 3.0 Reader, you can access the manual 
from the CD.  Using Windows Explorer, simply double-click on GFK1670.PDF in the 
\User Manual directory of the VersaPro CD.

If you don't have the latest copy of the Adobe Acrobat Reader, or are unsure of 
the version that you do have, a copy of the software is available on the VersaPro CD.  
Using Windows Explorer select Setup.exe in the \User Manual\Viewer\32Bit directory 
of your VersaPro CD.  This program will install the Adobe Acrobat reader, giving 
you access to the VersaPro Users Guide on-line. A paper copy of the VersaPro Users 
Guide, contact your local GE Fanuc distributor to order publication GFK-1670.

========== Hardware Compatibility Requirements ==========

VersaPro requires the following minimum CPU revision levels.  Please note that
firmware revision numbers greater than those shown below are supported by VersaPro.
In most cases firmware on existing CPU modules can be easily upgraded to meet these 
requirements:

Product Family		CPU Model Number	Required Revision (Firmware Revision
							is shown in parenthesis)
									

VersaMax Modular	IC200CPU001		AA(1.00),BC(1.20),BD(1.50),CD(1.50)
VersaMax Modular	IC200CPU002			AA(1.50)
VersaMax Modular	IC200CPU005			AA(2.00)
VersaMax Modular	IC200CPUE05			AA(2.00)


VersaMax Nano		IC200NDR001			AA(1.00)
VersaMax Nano		IC200NDR010			AA(1.00)
VersaMax Nano		IC200NDD010			AA(1.00)
VersaMax Nano		IC200NDD101			AA(1.00)
VersaMax Nano		IC200NAR001			AA(1.00)
VersaMax Nano		IC200NAL110			AA(2.00)
VersaMax Nano		IC200NAL211			AA(2.00)
VersaMax Nano		IC200NAR010			AA(2.00)
VersaMax Nano		IC200NAA010			AA(2.00)


VersaMax Micro		IC200UDR001			AA(1.00)
VersaMax Micro		IC200UDR002			AA(1.00)
VersaMax Micro		IC200UDR003			AA(1.00)
VersaMax Micro		IC200UAA003			AA(1.00)
VersaMax Micro		IC200UDD104			AA(1.00)
VersaMax Micro		IC200UDD112			AA(1.00)
VersaMax Micro		IC200UDR005			AA(1.00)
VersaMax Micro		IC200UAL004			AA(1.00)
VersaMax Micro		IC200UAL005			AA(1.00)
VersaMax Micro		IC200UAL006			AA(1.00)
VersaMax Micro		IC200UAA007			AA(1.00)
VersaMax Micro		IC200UDR005			AA(1.00)
VersaMax Micro		IC200UDR006			AA(1.00)
VersaMax Micro		IC200UDR010			AA(1.00)
VersaMax Micro		IC200UDD110			AA(1.00)
VersaMax Micro		IC200UDD120			AA(1.07)
VersaMax Micro		IC200UDD212			AA(1.00)
VersaMax Micro		IC200UAR014			AA(1.00)
VersaMax Micro		IC200UAR028			AA(1.00)

Series 90 Micro		IC693UDR001			R(3.10)
Series 90 Micro		IC693UDR002			R(3.10)
Series 90 Micro		IC693UAA003			R(3.10)
Series 90 Micro		IC693UDR005			R(3.10)
Series 90 Micro		IC693UAL006			R(3.10)
Series 90 Micro		IC693UAA007			R(3.10)
Series 90 Micro		IC693UDR010			S(3.10)


Series 90-30		IC693CPU311			L(4.40)
Series 90-30		IC693CPU313			L(4.40)
Series 90-30		IC693CPU321			L(4.40)
Series 90-30		IC693CPU323			L(4.40)
Series 90-30		IC693CPU331			CD(8.21)
							CA-CD(8.21)
							RA-CD(8.21)
Series 90-30		IC693CPU340			H(7.0)
Series 90-30		IC693CPU341			V(8.21)
							VCA(8.21)
							VRA(8.21)
Series 90-30		IC693CPU350		BC(9.01),BD(9.10),BE(10.0)
							RA-BA(8.01)
Series 90-30		IC693CPU351			GR(9.01)
							CA-GR(9.01)
Series 90-30		IC693CPU352		DG(9.01),DH(9.10),DJ(10.0)
							CA-DG(9.01)
Series 90-30		IC693CPU360		BC(9.01),BD(9.10),BE(10.0)
Series 90-30		IC693CPU363		AB(9.01),AC(9.10),AD(10.0)
Series 90-30		IC693CPU364		AB(9.01),AC(9.10),AD(10.0)
Series 90-30		IC693CPU374			 AA(11.0)

Series 90-70		IC697CPU731			 X(5.03)
Series 90-70		IC697CPU732			 G(5.03)
Series 90-70		IC697CPU771			 V(5.03)
Series 90-70		IC697CPU772			 L(5.03)
Series 90-70		IC697CPU781			JE(6.02)
Series 90-70		IC697CPU782			JE(6.02)
Series 90-70		IC697CPM914			GK(7.21)
Series 90-70		IC697CPM915			CF(7.21)
Series 90-70		IC697CPM924			EH(7.21)
Series 90-70		IC697CPM925			CF(7.21)
Series 90-70		IC697CPX772			AA(7.80)
Series 90-70		IC697CGR772			AA(7.85)
Series 90-70		IC697CPU780			 F(4.70)
Series 90-70		IC697CPX782			AA(7.80)
Series 90-70		IC697CPU788			DA(5.01)
Series 90-70		IC697CPU789			DA(5.01)
Series 90-70		IC697CPX928			AA(7.80)
Series 90-70		IC697CPX935			AA(7.80)
Series 90-70		IC697CGR935			CB(7.85)


90-70 CPUs not supported

Series 90-70		IC697CPM790			





Contact your local GE Fanuc Distributor for information on upgrading your Series 
90-30/90-70/VersaMax PLCs.  If your PLC is a model that supports flash memory (90-30 
models 350, 351,352, 360, 363, 364, 90-70 CPX CPUs, VersaMax CPUs), the latest version
of firmware is available at the GE Fanuc web site  www.gefanuc.com.
